When using industrial protocols, the minimum firmware version requirements for each device series and their corresponding Ethernet/IP and PROFINET configuration files are as follows:

| Model                                            | Firmware Version   | EthernetIP Configuration   | PROFINET Configuration File                              |
|---------------------------------------|----------------------|------------------------------|----------------------------------------------------|
| SC1000 Series Vision Sensor           | V1.0.0 and later    | smart_camera_sc1000.eds  | GSDML-V2.34-Hikvision-MV-20220313.xml       |
| SC2000E Series Vision Sensor          | V2.0.0 and later    | smart_camera_sc2000e.eds | GSDML-V2.34-Hikvision-MV-20220313.xml      |
| SC2000E (Mini) Series Vision Sensor   | V2.0.0 and later    | smart_camera_sc2000e.eds | GSDML-V2.34-Hikvision-MV-20220313.xml      |
| SC3000 Series Vision Sensor           | V2.0.0 and later    | smart_camera_sc3000.eds  | GSDML-V2.34-Hikvision-MV-20220313.xml       |
| SC3000X Series Vision Sensor          | V3.1.0 and later    | smart_camera_sc3000.eds  | GSDML-V2.34-Hikvision-MV-20220313.xml       |
| SC5000X Series Smart Camera           | V4.2.30 and later   | vm4xx.eds                         | GSDML-V2.34-Hikvision-VM4XX-20221014.xml |
| SC6000 Series Smart Camera            | V4.2.30 and later   | vm4xx.eds                         | GSDML-V2.34-Hikvision-VM4XX-20221014.xml |

Note:
-Configuration files can be obtained from the same folder as this document.
-Distribution models have the same configuration files as their corresponding baseline models.